Project 1415-29(b)

Window Replacement Project at Jackson County Library (Marianna Branch)

Jackson County Board of Commissioners

Addendum 3

Lighting Specifications for Jackson County Library

Marianna, FL.

* 15 day written prior approval on all Fixtures and Lamps
* Acuity / Lithonia Brand on all Fixtures
* 5year warranty on all LED fixtures
* 1 year warranty on all other fixtures.
* DSXF LED - 1.4 EPA rating, 100,000 hr. rated burn time, dimension’s 13 x 13 5/8”
* LED Lamps - direct T8 replacement and 120/227V rated, with safe end feature. 15 watt Frosted Lens, 3500k color.
* 2GTL4 /2GTL2 – EZ 1 EldoLed drivers, LED boards with plug and play wiring, 0-10v dimming, 3500k color
* LB surface – EZ1 EldoLed drivers, DLC rated, dimension’s 10” x 24”
* OLWX - IP 65 rated, 20 watt at 4000K , dimension’s 7 ½ x 8” x 3” depth
* RV8 - 3500 color at 3000 lumens, 42 watts rated , dimmable
* VAP – S.S mounting brackets, DLC rated, 4000 lumens, 6 kV surge protection, dimensions 8 ¼ x 4 1/8 x 54 ¾”
* WP2 – 50Dr Acrylic diffuser #12 with .125 up light Lens , dimension’s 7 3/16 x 3 ¼ x 48”
* ***The Contractor is responsible to pull all permits and arrange for final Inspection from the City/County.***
* ***Bids must include all labor, materials and taxes. The Board reserves the right to ask Contractor to agree to a direct purchase agreement if it so desires.***