**GRADER BLADES**

**BID SPECIFICATIONS**

3/4” w/overlay X 6” X 36” long section (curved) grader blade, with 5/8” bolt holes, a 3/8” x ¾” minimum

carbide bullnose insert, and a 1” carbide embedded overly on front of blade.

3/4" w/overlay X 6” X 48” long section (curved) grader blade, with 5/8” bolt holes, a 3/8” x ¾” minimum

carbide bullnose insert, and a 1” carbide embedded overly on front of blade.

FOB to Jackson County Road Department