**BOARD OF COUNTY COMMISSIONERS**

**JACKSON COUNTY, FLORIDA**

Project # 1819-24

**Jackson County Annual Grader Blade Contract**

**ADDENDUM 1**

Whenever there is a conflict between this addendum and the initial bid documents or plans, the addendum shall take precedence.

* The deadline for submittal of the sealed bids has been extended to Tuesday, June 10, 2019 at 2:00pm, CST
* The model of the John Deere is JD 672G and then CAT/12M3 for the Caterpillar.
* Estimated need of approx. 50 each annually
* Current delivery time is 7 days
* No bid Bond is required
* The specifications have been updated to the following

|  |  |
| --- | --- |
| **Cost (delivery included) for the following:*** 3/4” w/overlay x 6” x 36” long section (curved) grader blade, with 5/8” bolt holes, a 3/8” x ¾” minimum carbide bullnose insert, and a 1” carbide embedded overly on front of blade.
* 3/4" w/overlay x 6” x 48” long section (curved) grader blade, with 5/8” bolt holes, a 3/8” x ¾” minimum carbide bullnose insert, and a 1” carbide embedded overly on front of blade.
* 3/4” w/overlay x 6” x 36” long section (curved) grader blade, with 3/4” bolt holes, a 3/8” x ¾” minimum carbide bullnose insert, and a 1” carbide embedded overly on front of blade.
* 3/4" w/overlay x 6” x 48” long section (curved) grader blade, with 3/4” bolt holes, a 3/8” x ¾” minimum carbide bullnose insert, and a 1” carbide embedded overly on front of blade.

**Number of days required for delivery**--------------------------------- \_\_\_\_\_\_\_\_\_\_\_\_ |   $\_\_\_\_\_\_\_\_\_\_\_\_each  $\_\_\_\_\_\_\_\_\_\_\_ each  $\_\_\_\_\_\_\_\_\_\_\_ each $\_\_\_\_\_\_\_\_\_\_\_\_each |
|  |  |
|  |  |
|  |  |
|  |  |